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- High precision weight class F1, Knob or Wire or
sheet weights

-Special stainless steel highly polished, in box 4

-With DAKKS calibration certificate
-Nominal weights:100mg

£ fe High precision weight class F1, Knob or Wire or
sheet weights
-Special stainless steel highly polished, in box 4
-With DAKKS calibration certificate
-Nominal weights:500mg
3 | Tweezer, Straight tips 2
4 | Soft brush 2
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